We are releasing the latest NDOR software update.
The firmware version is v1.3.6, and the backend version is v1.1.3.

Please proceed with the upgrade only if you are using firmware version v1.2.x or higher. (Firmware v1.1.4 is also supported)

=========================================
To update, select the attached "NDOR_fw-v1.3.6-be-v1.1.3.srv" file on the [Firmware Update] page of the web UI.
Note: Do not turn off the device power forcibly before the software has completed the update and the device starts functioning again.
During the update, the LCD screen will remain black for approximately 1 minute and 40 seconds.
After the update, please refresh the login page on the WEB UI the first time you access it. (Ctrl+F5)

Key updates are as follows:

[ fw-v1.3.6-be-v1.1.3 ]

Added Time Zone, NTP Server settings, and time setting API (New [SYSTEM] tab added to WebUI)

Display year in four digits for saved file names

Added automatic recording start/stop option based on streaming activity

[ fw-v1.3.5-be-v1.1.2 ]

Fixed issue where device stopped working during long recordings/saving

[ fw-v1.3.4-be-v1.1.2 ]

Added RTSP server functionality

Changed audio capture method

Fixed issue where output audio was distorted when switching audio inputs

Fixed issue where only part of the input video was displayed when input resolution changed

Added setServerPort (HTTP API) for changing the backend server connection port

[ fw-v1.2.6-be-v1.1.1 ]

Fixed issue where screen would be corrupted during playback due to unexpected frame drops during encoding

[ fw-v1.2.5-be-v1.1.1 ]

Improved quality degradation when encoding at 720P resolution

Fixed LCD and output video corruption caused by resolution setting errors when changing input video sources

Fixed issue where noise (font image) appeared at the top of the output video when encoding at 4K resolution

[ fw-v1.1.4-be-v1.1.1 ]

Upgraded to NDI version 6

[ fw-v1.1.3-be-v1.1.1 ]

Created a 640x360 snapshot image for previewing input video every 3 seconds

Example path: http://[NDOR IP Address]/preview/snapshot.jpg

Added [REBOOT] button to the system information section on the HOME page of the WEB UI

[ fw-v1.1.2-be-v1.1.0 ]

Displayed "WAIT..." string until file saving is complete while stopping recording

Improved file overwriting (Overwrite) method in case of insufficient storage during recording

[ fw-v1.1.1-be-v1.1.0 ]

Fixed bug where stream output temporarily stopped while stopping recording

Improved file overwriting (Overwrite) method in case of insufficient storage during recording

Adjusted the brightness of the input video to be brighter than before

[ fw-v1.1.0-be-v1.1.0 ]

HTTP API support

Supported 14 APIs according to v1 draft

Fixed bug where audio input change via WEB UI was not properly reflected on the device’s OSD

Changed the string for SD card from "SDC" to "SD" on the [Recording] page of the WEB UI