Release of the latest NDOR software update.
The firmware version is v1.3.9, and the backend version is v1.1.7.

Please upgrade only if your current firmware is v1.2.x or later (Firmware v1.1.4 is supported).

======================================================================
To update, select the attached "NDOR_fw-v1.3.9-be-v1.1.7.srv" file through the [Firmware Update] page in the web UI.
Note: Do not power off the device forcefully before the software update completes and the device resumes operation.
During the update, the LCD screen will be black for approximately 1 minute and 40 seconds.
After the update, please perform a REFRESH on the login page in the WEB UI the first time (Ctrl+F5).

Key updates are as follows:

[ fw-v1.3.9-be-v1.1.7 ]

Improved AV synchronization mechanism

RTMPS streaming support

[ fw-v1.3.7-be-v1.1.5 ]

Support for TS file format recording

Added the ability to display and set the system's current time in the WebUI

Increased the number of NDI Discovery Server settings to 2

[ fw-v1.3.6-be-v1.1.3 ]

Added Time Zone, NTP Server settings, and time-setting API (added [SYSTEM] tab to WebUI)

Displayed the year in four digits in saved file names

Added an option to start/stop automatic recording based on streaming behavior

[ fw-v1.3.5-be-v1.1.2 ]

Fixed an issue where the device stopped functioning during long-duration recording/storage

[ fw-v1.3.4-be-v1.1.2 ]

Added RTSP server functionality

Changed audio capture method

Fixed an issue where output audio was corrupted when switching audio input

Fixed an issue where only part of the input video was output when the input resolution changed

Added setServerPort (HTTP API) for changing the backend server’s connection port

[ fw-v1.2.6-be-v1.1.1 ]

Improved the issue where the output video would break during playback due to unexpected frame drops during encoding

[ fw-v1.2.5-be-v1.1.1 ]

Improved quality degradation when encoding at 720P resolution

Fixed an issue where the LCD and output video would break when changing the input video source due to resolution setting errors

Fixed an issue where noise (font images) would appear at the top of the output video when encoding at 4K resolution

[ fw-v1.1.4-be-v1.1.1 ]

Upgraded to NDI version 6

[ fw-v1.1.3-be-v1.1.1 ]

Created a 640x360 size snapshot image every 3 seconds for previewing the input video

Example path: http://[NDOR IP Address]/preview/snapshot.jpg

Added a [REBOOT] button to the system information section on the WEB UI’s HOME page

[ fw-v1.1.2-be-v1.1.0 ]

Displayed the "WAIT..." string until file storage is complete when stopping recording

Improved the file overwrite method due to insufficient storage space during recording

[ fw-v1.1.1-be-v1.1.0 ]

Fixed a bug where stream output stopped temporarily while stopping recording

Improved the file overwrite method due to insufficient storage space during recording

Adjusted the brightness of the input video to be brighter than before

[ fw-v1.1.0-be-v1.1.0 ]

Added HTTP API support

Supported 14 APIs in line with version 1 draft

Fixed a bug where audio input changes via the WEB UI were not displayed correctly on the device’s OSD

Changed the SD card string from "SDC" to "SD" on the WEB UI’s [Recording] page

Please test it and contact us if you encounter any issues or have other inquiries.

That’s all.